|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Appendix. Traditional Drywall productivity on Veidekke’s project (per Apartment). | | | | |
| Productivity (h/m2) | **Apartment 4** | **Apartment 6** | **Apartment 5** | **Average** |
| Drywall side 1 (including studs) | 0.10 | 0.12 | 0.11 | 0.11 |
| Drywall side 2 | 0.14 | - | - | 0.14 |
| Electrical | 0.10 | 0.10 | - | 0.10 |
| TOTAL (w/o electrical) | 0.24 |  |  | 0.25 |